**CompTIA A+**

To watch the below video, you need to right click on the Hyperlink just below the highlighted task in red color and select the Open Hyperlink option. It will take you to the YouTube where you can watch the concerned video.

You are required to watch the video and answer the Questions asked below.

You need to type answers in the row indicated with “Ans.”

|  |  |
| --- | --- |
| **Printer maintenance**  <https://drive.google.com/file/d/14DaMaAa6NXR2ehhcNipR_cY1j9vo8N0z/view?usp=sharing> | |
| 1 | What is the maintenance done on a laser printer? |
| Ans. | UNPLUGPRINTER , REMOVE PAPER TRAY , CLEAN PRINTER TONNER |
| 2 | What is the maintenance done on a thermal printer? |
| Ans. | should inspect the interior area after every four rolls of media. Remove any dirt and lint from the interior of the printer using a soft bristle brush and/or vacuum cleaner. Don't forget to clean the Printhead and Platen Roller! |
| 3 | What is the maintenance done on an impact printer? |
| Ans. | Keeping an impact printer clean is the primary maintenance required, besides replacing the paper and replacing the ink ribbon. |
| 4 | What is the maintenance done on an inkjet printer? |
| Ans. | * Nozzle Checking and Head Cleaning. ... |
| 5 | Why do we need to print test page? |
| Ans. | PEEGE SETUP AND ALLIMENT |